IPASS

**ColorFinder**

**Using TCS34725 Module**

WS2812B

The colorfinder uses a TCS34725 colorsensor to recognise colors and sends the data to a WS2812B RGB ledstrip to display the color.

A close-up of a circuit board

Description automatically generated with low confidence

Zoë van de Pol

Qr code

Description automatically generated

TCS34725

Library

A library that can be

used with the TCS34725

colorsensor that uses I2C comminucation

jj